FOSROC INC -- PRECO PATCH -- 5610-00N048268

===================== Product Identification =====================

Product ID:PRECO PATCH

MSDS Date:04/08/1993

FSC:5610

NIIN:00N048268

MSDS Number: BVCCP

=== Responsible Party ===

Company Name:FOSROC INC

Address:55 SKYLINE DR

City:PLAINVIEW

State:NY

ZIP:11803

Country:US

Info Phone Num:800-645-3954

Emergency Phone Num:800-424-9300 (CHEMTREC)

CAGE:GO196

=== Contractor Identification ===

Company Name:FOSROC INC

Address:55 SKYLINE DRIVE

City:PLAINVIEW

State:NY

ZIP:11803

Country:US

Phone:516-935-9100

CAGE:GO196

============= Composition/Information on Ingredients =============

Ingred Name:PORTLAND CEMENT

CAS:65997-15-1

RTECS #:VV8770000

OSHA PEL:15 MG/M3 TDUST

ACGIH TLV:10 MG/M3 TDUST

Ingred Name:SILICA, CRYSTALLINE - QUARTZ; (SILICA SAND)

CAS:14808-60-7

RTECS #:VV7330000

OSHA PEL:0.1 MG/M3 RDUST

ACGIH TLV:0.1 MG/M3 RDUST

Ingred Name:CALCIUM OXIDE; (LIME)

CAS:1305-78-8

RTECS #:EW3100000

OSHA PEL:5 MG/M3

ACGIH TLV:2 MG/M3

===================== Hazards Identification =====================

LD50 LC50 Mixture:NONE SPECIFIED BY MANUFACTURER.

Routes of Entry: Inhalation:YES Skin:NO Ingestion:NO

Reports of Carcinogenicity:NTP:YES IARC:YES OSHA:NO

Health Hazards Acute and Chronic:EYES:CAN CAUSE IRRITATION, REDNESS,

TEARING, BLURRED VISION. SKIN:CAN CAUSE IRRITATION, BURNS.

INHALATION:CAN CAUSE INJURY TO LUNGS. INGESTION:CAN CAUSE

GASTROINTESTINAL IRRITATION. CHRONIC: SILICOSIS MAY DEVELOP AFTER

PROLONGED EXPOSURE.

Explanation of Carcinogenicity:SILICA, CRYSTALLINE-QUARTZ:IARC

MONOGRAPHS, SUPPLEMENT. VOL 7, PG 341, 1987:GROUP 2A. NTP 6TH

ANNUAL REPORT ON (SUPDAT)

Effects of Overexposure:SEE HEALTH HAZARDS.

Medical Cond Aggravated by Exposure:NONE SPECIFIED BY MANUFACTURER.

======================= First Aid Measures =======================

First Aid:EYES: FLUSH WITH LARGE AMOUNTS OF WATER, LIFTING UPPER &

LOWER LIDS OCCASIONALLY. SEE MD IMMEDIATELY. SKIN: THOROUGHLY WASH

EXPOSED AREA WITH SOAP & WATER. REMOVE CONTAMINATED CLOTHING.

LAUNDER CONTAM INATED CLOTHING BEFORE RE-USE. INHALATION: KEEP

PERSON WARM, QUIET & SEE MD IMMEDIATELY. INGESTION: DO NOT INDUCE

VOMITING. KEEP PERSON WARM, QUIET & SEE MD IMMEDIATELY.

===================== Fire Fighting Measures =====================

Extinguishing Media:MEDIA SUITABLE FOR SURROUNDING FIRE .

NON-COMBUSTIBLE.

Fire Fighting Procedures:USE NIOSH/MSHA APPROVED SCBA AND FULL

PROTECTIVE EQUIPMENT .

================== Accidental Release Measures ==================

Spill Release Procedures:SMALL SPILL: CLEAN UP BY USE OF DUSTLESS

METHODS.

Neutralizing Agent:NONE SPECIFIED BY MANUFACTURER.

====================== Handling and Storage ======================

Handling and Storage Precautions:CNTNRS OF MATL MAY BE HAZ WHEN

EMPTIED. SINCE EMPTIED CNTNRS RETAIN PROD RESIDUES (VAP, LIQ &/OR

SOLID), ALL HAZ PREC GIVEN IN MSDS MUST BE OBSERVED.

Other Precautions:KEEP OUT OF REACH OF CHILDREN.

============= Exposure Controls/Personal Protection =============

Respiratory Protection:NIOSH/MSHA RESPIRATOR (DUST FILTER TYPE IN

COMPLIANCE WITH OSHA STD 29 CFR 1910.134).

Ventilation:PROVIDE SUFFICIENT MECHANICAL (GENERAL) AND/OR LOCAL

EXHAUST VENTILATION TO MAINTAIN EXPOSURE BELOW TLV'S.

Protective Gloves:CHEMICAL RESISTANT SUCH AS BUNA-N.

Eye Protection:ANSI APPVD CHEM WORK GOGG .

Other Protective Equipment:TO PREVENT REPEATED OR PROLONGED SKIN

CONTACT WEAR IMPERVIOUS CLOTHING AND BOOTS.

Work Hygienic Practices:NONE SPECIFIED BY MANUFACTURER.

Supplemental Safety and Health

EXPLAN OF CARCIN:CARCINOGENS, 1991:ANTICPATED TO BE CARCINOGEN.

================== Physical/Chemical Properties ==================

HCC:N1

Vapor Density:HVR/AIR

Evaporation Rate & Reference:SLOWER THAN ETHER

Appearance and Odor:GREY POWDER WITH NO ODOR.

Percent Volatiles by Volume:0

================= Stability and Reactivity Data =================

Stability Indicator/Materials to Avoid:YES

AVOID CONTACT WITH ACID MINERALS.

Stability Condition to Avoid:NONE SPECIFIED BY MANUFACTURER.

Hazardous Decomposition Products:MAY FORM TOXIC MATERIALS - CALCIUM

OXIDES, SILICATES AND SULFATE.

==================== Disposal Considerations ====================

Waste Disposal Methods:DISPOSE OF IN ACCORDANCE WITH LOCAL, STATE AND

FEDERAL REGULATIONS.

Disclaimer (provided with this information by the compiling agencies):

This information is formulated for use by elements of the Department

of Defense. The United States of America in no manner whatsoever,

expressly or implied, warrants this information to be accurate and

disclaims all liability for its use. Any person utilizing this

document should seek competent professional advice to verify and

assume responsibility for the suitability of this information to their

particular situation.