RAECO INC -- RAECO-SET THIN SET MORTAR POWDER -- 5610-00N047103

===================== Product Identification =====================

Product ID:RAECO-SET THIN SET MORTAR POWDER

MSDS Date:04/01/1985

FSC:5610

NIIN:00N047103

MSDS Number: BSKHB

=== Responsible Party ===

Company Name:RAECO INC

Box:80545

City:SEATTLE

State:WA

ZIP:98108

Country:US

Info Phone Num:206-763-1335

Emergency Phone Num:206-763-1335

CAGE:2A957

=== Contractor Identification ===

Company Name:RAECO INC

Box:City:SEATTLE

State:WA

ZIP:98108

Country:US

Phone:206-763-1335

CAGE:2A957

============= Composition/Information on Ingredients =============

Ingred Name:DEHYDRATING POWDERS; (BLENDED DEHYDRATING POWDERS)

(BUILDING CEMENTS)

OSHA PEL:N/K

ACGIH TLV:N/K

Ingred Name:SILICA SAND; (SILICA SANDS)

OSHA PEL:N/K

ACGIH TLV:N/K

===================== Hazards Identification =====================

LD50 LC50 Mixture:NONE SPECIFIED BY MANUFACTURER.

Routes of Entry: Inhalation:YES Skin:NO Ingestion:NO

Reports of Carcinogenicity:NTP:NO IARC:NO OSHA:NO

Health Hazards Acute and Chronic:ACUTE: WET MIXTURE CAN DRY SKIN AND

CAUSE ALKALI BURNS. DRY DUST CAN IRRITATE EYES AND UPPER

RESPIRATORY SYSTEM. CHRONIC: DUST CAN CAUSE INFLAMMATION OF LINING

TISSUE OF INTERIOR OF NOSE & INFLAMMATIO N OF CORNEA.

HYPERSENSITIVE INDIVIDUALSMAY DEVELOP AN ALLERGIC DERMATITIS. EFTS

OF OVEREXP: (EFTS OF OVEREXP)

Explanation of Carcinogenicity:NOT RELEVANT

Effects of Overexposure:HLTH HAZ: PNEUMOCONIOSIS-PULMONARY FIBROSIS

FROM LONG-TERM EXPOSURE TO RESPIRABLE DUST.

======================= First Aid Measures =======================

First Aid:EYES: IRRIGATE WITH WATER FOR AT LEAST 15 MINUTES. SKIN: WASH

AFFECTED AREAS OF BODY WITH SOAP AND WATER. INHAL: REMOVE TO FRESH

AIR. SUPPORT BRTHG (GIVE O2/ARTF RESP) . INGEST: CALL MD IMMED (F P

N).

===================== Fire Fighting Measures =====================

Extinguishing Media:NOT COMBUSTIBLE. MEDIA SUITABLE FOR SURROUNDING

FIRE .

Fire Fighting Procedures:WEAR NIOSH/MSHA APPROVED SCBA AND FULL

PROTECTIVE EQUIPMENT .

Unusual Fire/Explosion Hazard:NONE KNOWN.

================== Accidental Release Measures ==================

Spill Release Procedures:USE DRY CLEAN-UP METHODS (SWEEP/VACUUM) THAT

DO NOT DISPERSE DUST INTO AIR. AVOID BREATHING DUST.

Neutralizing Agent:NONE SPECIFIED BY MANUFACTURER.

====================== Handling and Storage ======================

Handling and Storage Precautions:STORE IN DRY AREAS. AVOID HIGH HEAT

AND COLD.

Other Precautions:PRACTICE REASONABLE PRECAUTIONS TO AVOID BREATHING

DUST AND REPEATED OR PROLONGED SKIN CONTACT. FOLLOW OSHA STANDARDS.

PRECAUTIONS MUST BE OBSERVED BECAUSE CEMENT BURNS OCCUR W/LITTLE

WARNING-LITTLE H EAT IS SENSED.

============= Exposure Controls/Personal Protection =============

Respiratory Protection:INDUSTRY ENVIRONMENTS, USE OF A NIOSH/MSHA

APPROVED RESPIRATOR RECOMMENDED.

Ventilation:LOCAL EXHAUST: TO CONTROL AIRBORNE DUST LEVELS.

Protective Gloves:CLOTH.

Eye Protection:TIGHT FITTING GOGGLES.

Other Protective Equipment:BARRIER CREAMS, BOOTS & CLOTHING TO PROTECT

FROM CONTACT OF WET MIXTURE.

Work Hygienic Practices:IMMED AFTER WORKING W/MATL, WORKERS SHOULD

SHOWER WITH SOAP AND WATER.

Supplemental Safety and Health

NONE SPECIFIED BY MANUFACTURER.

================== Physical/Chemical Properties ==================

HCC:T6

Solubility in Water:SLIGHT (0.1-1%)

Appearance and Odor:GREYISH, FINE GRANULAR POWDER

================= Stability and Reactivity Data =================

Stability Indicator/Materials to Avoid:YES

NONE.

Stability Condition to Avoid:NONE KNOWN.

Hazardous Decomposition Products:NONE.

==================== Disposal Considerations ====================

Waste Disposal Methods:SAME AS FOR CEMENTITIOUS MATERIALS. DISPOSE OF

AS A COMMON WASTE. DISPOSE OF I/A/W FEDERAL, STATE AND LOCAL

REGULATIONS .

Disclaimer (provided with this information by the compiling agencies):

This information is formulated for use by elements of the Department

of Defense. The United States of America in no manner whatsoever,

expressly or implied, warrants this information to be accurate and

disclaims all liability for its use. Any person utilizing this

document should seek competent professional advice to verify and

assume responsibility for the suitability of this information to their

particular situation.